|  |
| --- |
| **FEATURES** |
| **Platform height elevated 9,68 m** |
| **Overall width 1,17 m** |
| **Platform capacity 320 kg** |
| **Roll out deck extension 1,27 m** |
| **Fold-down handrails** |
| **Lanyard attach points** |
| **Proportional hydrostatic drive control with thumb steer** |
| **Proportional lift up** |
| **GLOBEN, S.L.**  C/Germán Bernácer 95  Elche Parque Empresarial  Apdo. De Correos 5154·03203 **ELCHE** (Alicante)  Telf. **966 299 599** · Móvil 673 823 100  GLOBEN.jpgFax 965 680 523 · [info@globen.es](mailto:info@globen.es)  **www.globen.es** |



**ELECTRIC SCISSOR LIFT**

**JLG 3246ES 12M HEIGHT**

|  |  |
| --- | --- |
| DIMENSIONS | |
| A. Platform height (elevated) | 9.68 m |
| B. Platform height (lowered) | 1.26 m |
| C. Platform railing height | 1.10 m |
| D. Overall height rails lowered | 1.97 m |
| E. Platform size | 1.12 m x 2.50 m |
| F. Platform extension | 1.27 m |
| G. Overall width | 1.17 m |
| H. Overall height | 2.50 m |
| I. Wheelbase | 2.09 m |
| J. Ground clearance | 0.13 m |
| Platform capacity1 | 320 kg |
| Capacity on platform extension | 120 kg |
| Lift/lower time | 50/60 sec. |
| Maximum drive height | 9.68 m |
| Platform weight | 2,870 kg |
| Ground bearing pressure | 6.90 kg/cm2 |
| Drive speed lowered | 4.0 km/h |
| Drive speed elevated | 0.8 km/h |
| Gradeability | 25% |
| Turning radius (intern) | 0 |
| Turning radius (extern) | 2.41 m |
| Tires | 406 x 125 |
| Brakes | Electric, automatic friction |
| Drive | 24V electric 6 kW |
| Batteries | 4 x 6V 220 A/hr |
| Charger | (120/240V – 50/60HZ) 20 amp automatic |
| Electric motor | 3 kW |
| Hydraulic reservoir | 20.0 L |

**1Capabilities provided with a maximum of 2 people inside.**

