**ENGINE POWERED SCISSOR LIFT**

**JLG 500RTS 17M HEIGHT**

****

****

**GLOBEN, S.L.**

C/Germán Bernácer 95

Elche Parque Empresarial


Apdo. De Correos 5154·03203 **ELCHE** (Alicante)

Telf. **966 299 599** · Móvil 673 823 100

Fax 965 680 523 · [info@globen.es](mailto:info@globen.es)

**www.globen.es**

|  |  |
| --- | --- |
| DIMENSIONS | |
| **A.** Platform height (elevated) | 15.24 m |
| **B.** Platform height (lowered) | 2.03 m |
| C. Platform railing height1 | 1.10 m |
| D. Overall height (rails lowered)1 | 2.45 m |
| E. Platform size | 1.80 m x 4.27 m |
| **F.** Platform extension2 | 1.23 m |
| **G. Overall width** | 2.29 m |
| **H. Overall length** | 4.70 m |
| **I. Wheelbase** | 3.10 m |
| **J. Ground clearance** | 0.30 m |
| Platform capacity | 1,134 kg |
| Capacity with dual extension | 910 kg |
| Capacity on platfom extension | 265 kg |
| Lift/lower time | 72/72 sec. |
| Maximum drive height | 6.99 m |
| Platform extension front | (Optional) hydraulic |
| Platform extension rear | (Optional) hydraulic |
| Weight3 | 8,200 kg |
| Speed 4x2x2 | 5.6 km/h |
| Speed 4x4x2 (optional) | 4.5 km/h |
| Gradeability 4x2x2 | 35% |
| Gradeability 4x4x2 (opcional) | 45% |
| Turning radius (intern) (simple direction) | 4.01 m |
| Turning radius (intern) (double direction) | 1.98 m |
| Turning radius (extern) (simple direction) | 5.72 m |
| Turning radius (extern) (double direction) | 3.68 m |
| Axle (optional) | 0.20 m |
| Tires | 12 x 16.5 |
| Diesel fuel engine | 30 kW Deutz F3L1011 |
| Fuel tank capacity | 56.8 L |
| Hydraulic reservoir | 140 L |

1 With the optional sliding side increases the height at 0.08 m.   
2 Optionally 500RTS model with hydraulic sliding single or double side 1.23 m.   
3 Weights and dimensions may vary due to each country's regulations or the options.

