                  GLOBEN, S.L. – ELECTRIC SCISSOR LIFT JLG M3369 14M HEIGHT-

	RESUMEN ESPÉCIFICACIONES

	Platform height elevated 10,06 m

	Overall width 1,75 m

	Platform capacity 450 kg

	Roll out deck extension de 0,91 m

	Fold-down handrails

	Lanyard attach points

	Proportional hydrostatic drive control with thumb steer

	Proportional lift up

	Choice oof two speeds driving

	Hydraulic leveling jacks
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	DIMENSIONS

	A. Platform height (elevated) 
	10.06 m

	B. Platform height (lowered) 
	1.69 m

	C. Platform railing height1 
	1.10 m

	D. Overall height rails lowered
	1.98 m

	E. Platform size 
	1.65 m x 2.92 m

	F. Platform extension 
	0.91 m

	G. Overall width 
	1.75 m

	H. Overal length 2 
	3.07 m

	I. Wheelbase 
	2.32 m

	J. Ground clearance 
	0.20 m

	Platform capacity 
	450 kg

	Capacity on platform extension
	120 kg

	Lift/lower time 
	38/42 sec.

	Maximum drive height 
	10.06 m

	Platform weight 1 2 
	5,250 kg

	Ground bearing pressure 
	8.1 kg/cm2

	Drive speed (lowered) 
	4.8 km/h

	Drive speed (elevated) 
	0.8 km/h

	Gradeability 
	35%

	Turning radius (intern) 
	2.29 m

	Turning radius (extern) 
	4.88 m

	Tires 
	240/55-17.5

	Brakes
	Spring applied hydraulically released discs

	Motor
	Electric

	Hydraulic motor pump
	Electric motor

	Batteries 
	8 x 6V 370 A/hr

	Charger (120/240V - 50/60HZ)
	23 amp SCR automatic

	Hydraulic pump 
	Gear pump

	Hydraulic reservoir 
	32 L

	Automatic generator
	15 L


1 Certain options or country standards may increase weight and / or dimensions.
2The dimensions of the two optional stabilizers are: 3.73 m long, 1.75 m wide + 400 kg weight.
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